Product	Name	Organoid® RELAX on flax backing	
	Article number	RLX0000085FVPRW	
Producer	Address	ORGANOID TECHNOLOGIES GMBH
Nesselgarten 422 / Top 5
A-6500 Fließ
Österreich
	
Description and applications	Name	Organoid® RELAX on flax backing	
	Description	Natural plant material in full coverage on natural non-woven flax backing produced climate neutral in Tyrol	
	Applications	As wallpaper  
As a compound in wood-working
	
Plant material and density	Plant material	Soothing herbal mixture	
	Density	Premium density, full coverage
	
Size and weight	Size	Rolled goods, width 1 360 mm 	
	Thickness	0.8 mm	
	Weight	720 g/m²
	
Product requirements	Food-safety	Binding agent safe for usage in contact with food in accordance with EU-regulation 1935/2004
	
Backing material	Material	Natural, non-woven flax fleece	
	Properties	Unbleached and breathable
from a renewable material
Contains 100% flax	
		Certified OEKO-TEX 100
Tensile strength in accordance with ISO 9073-3:
MD N/5cm 65
CD N/5cm 45
	
Technical implementation	Cut	Use scissors, a cutter or a plotter	
	Edges	Allow for imperfections 1-2 mm around the edges	
	How to install	As wallpaper:
-Wall-pasting technique: Apply glue directly on the wall, apply wallpaper vertically and press on using a rubber roller
-Double cut: Each panel overlaps with the one next to it (approx. 2 cm) 
-Free match: The naturally scattered materials do not require matching patterns between panels

As a compound in wood-working
-Process with normal wood-working machinery
-Glue (e.g. white glue) is applied onto the wooden materials, as the fleece absorbs moisture and glue stains may appear on the front if glue is applied to the fleece
-Cover the natural surface with the enclosed separating paper
-Guidelines:
Max. pressing temperature. 60°C
Max. pressure 1 kg/cm²
Glue application: approx. 100 g/m²
Pressing time: approx. 15 minutes

Pre-trials and tests are recommended
	
	Glue recommendations	As wallpaper:
•	Methylan Direct Kleister Vliestapeten
•	Pufas Glasgewebe- und Vlieskleber GK,
•	Pufas Sicherheitskleister SK,
•	AURO Wandbelagskleber Nr. 391 (ecological glue),
•	Universalkleber für Vliestapeten
•	Nr. 380 (ecological glue) 
As a compound in wood-working:
•	White glue
	
	Pay attention to	Surface must be clean, dry, weight-bearing, evenly absorbent, smooth, dust-free and neutral in colour. Recently plastered walls must be fully dried. Highly absorbent walls must be prepared with a suitable base. 

For sensitive wood-working applications, use a counter-balance (enclosed on request). Symmetrical construction is recommended, which means using the same surface on the front and back side.

Acclimatisation of Organoid natural surfaces: 
- Bring product to room temperature before unpacking 
- Store product protected from light, at about 20°C and 30-60 % relative humidity.
- Storage:
•	Rolled goods: hanging system (e.g. paternoster)
•	Single panels: horizontal position (e.g. drawer system)	
	Processing guidelines available at:	https://organoid.corestad.com/verarbeitung/
(= current link)